; Copyright (C) [2011] OPPO Corporation
;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer           = 02/11/2015,4.5.0000.00000
CatalogFile.NTx86   = androidwinusb86.cat
CatalogFile.NTamd64 = androidwinusba64.cat

;
; This section seems to be required for WinUsb driver installation.
; If this section is removed the installer will report an error
; "Required section not found in INF file".
;
[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[Manufacturer]
%ProviderName% = OPPO, NTx86, NTamd64

[OPPO.NTx86]
; HTC Dream
%SingleAdbInterface%        = USB_Install, USB\VID_0BB4&PID_0C01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0C02&MI_01
%SingleBootLoaderInterface% = USB_Install, USB\VID_0BB4&PID_0FFF

; HTC Magic
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0C03&MI_01

; Moto Sholes
%SingleAdbInterface%        = USB_Install, USB\VID_22B8&PID_41DB
%CompositeAdbInterface%     = USB_Install, USB\VID_22B8&PID_41DB&MI_01

; Google NexusOne
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001&REV_0404
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001

; MT65xx
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0004&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0007&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2010&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_201B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2025&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2021&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2022&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2023&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2024&MI_04
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4EE7

; OPPO
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2765&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2766&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2767&MI_00
%SingleAdbInterface%        = USB_Install, USB\VID_22D9&PID_2769
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2769&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22d9&PID_2770&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2772&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2774&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2775&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2776&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2777&MI_01	
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2778&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2779&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_277A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_277B&MI_06
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2782&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_0C03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2028&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2D01&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2D03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2D05&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9031&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9091&MI_03
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D
%SingleBootLoaderInterface% = USB_Install,USB\VID_18D1&PID_4EE2&MI_01
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE2&REV_0409&MI_01
;mtk
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2003&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2005&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2006&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2010&MI_02
%SingleAdbInterface%        = USB_Install, USB\VID_0E8D&PID_201C
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_201D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_201B&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_0E8D&PID_2024
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2025&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2026&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2027&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2028&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_202E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_202F&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2030&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2040&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2041&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2044&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2061&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2062&MI_02

;C2K related
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2032&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2034&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2035&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2037&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2039&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2050&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2053&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2054&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2063&MI_07
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2064&MI_02


;MIDI related
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2048&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2049&MI_02

;MBIM related
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2056&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2057&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2059&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205F&MI_01
;mtk end 

;oppo copy from mtk
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2003&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2005&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2006&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2010&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE9&MI_02

;replace by oppo 2769 %SingleAdbInterface%        = USB_Install, USB\VID_22D9&PID_201C
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_201D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_201B&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_22D9&PID_2024
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2025&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2026&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2027&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2028&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_202E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_202F&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2030&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2040&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2041&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2044&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2061&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2062&MI_02

;C2K related
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2032&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2034&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2035&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2037&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2039&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2050&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2053&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2054&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2063&MI_07
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2064&MI_02


;MIDI related
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2048&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2049&MI_02

;MBIM related
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2056&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2057&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2059&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205F&MI_01
;;oppo copy from mtk end 

;oppo new add
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90B4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90B6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_903A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9060&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9082&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_908C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90D1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_901F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90B8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90D3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2767&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2006&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_2D03&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2048&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2049&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2032&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2034&MI_03
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0&REV_0414
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0
;oppo new add end 

;Unisoc add SPRD Adb
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4002&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4003&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4012&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4013&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4022&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4023&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4026&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4028&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4029&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4030&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4032&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4033&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4D01&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5A5B&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D01&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D04&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D06&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D21&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D23&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D24&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D25&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D27&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D29&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D31&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D34&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A002&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A002&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A012&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A012&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A022&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A022&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD21&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD21&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD24&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD24&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D001
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D002
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4002&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4003&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4012&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4013&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4022&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4023&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4026&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4028&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4029&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4030&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4032&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4033&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4D01&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5A5B&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D01&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D04&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D06&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D21&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D23&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D24&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D25&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D27&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D29&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D31&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D34&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_A002&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_A002&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_A012&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_A012&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_A022&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_A022&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_AD21&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_AD21&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_AD24&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_AD24&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_D001
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_D002
; GOOGLE Adb
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_0FFF
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D06&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D07&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D08&MI_01
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE7&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE8&MI_00
%SingleBootLoaderInterface%  = USB_Install, USB\VID_22d9&PID_0FFF
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_2D06&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_2D07&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_2D08&MI_01
%SingleBootLoaderInterface%  = USB_Install, USB\VID_22d9&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_200E&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_200E&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4EE7&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4EE8&MI_00

;add plus
;14041
%SingleAdbInterface%        = USB_Install, USB\VID_22D9&PID_2769
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2769&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9031&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2765&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2766&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2767&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2772&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2774&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2775&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9025&MI_01
;14049
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D       ;fastboot
%SingleBootLoaderInterface% = USB_Install, USB\VID_2A70&PID_D00D       ;oem fastboot
%SingleAdbInterface%        = USB_Install, USB\VID_2A70&PID_4EE7       ;adb
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9031&MI_02 ;default
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9091&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9039&MI_01 ;mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_904E&MI_01 ;ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9011&MI_02 ;mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9012&MI_02 ;mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_901C&MI_00 ;adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9015&MI_01 ;mtp,adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9024&MI_02 ;rndis,adb

[OPPO.NTamd64]
; HTC Dream
%SingleAdbInterface%        = USB_Install, USB\VID_0BB4&PID_0C01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0C02&MI_01
%SingleBootLoaderInterface% = USB_Install, USB\VID_0BB4&PID_0FFF

; HTC Magic
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0C03&MI_01

; Moto Sholes
%SingleAdbInterface%        = USB_Install, USB\VID_22B8&PID_41DB
%CompositeAdbInterface%     = USB_Install, USB\VID_22B8&PID_41DB&MI_01

; Google NexusOne
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001&REV_0404
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001


; MT65xx
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0004&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0007&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2010&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_201B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2025&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2021&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2022&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2023&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_2024&MI_04
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4EE7

; OPPO
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2765&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2766&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2767&MI_00
%SingleAdbInterface%        = USB_Install, USB\VID_22D9&PID_2769
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2769&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22d9&PID_2770&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2772&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2774&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2775&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2776&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2777&MI_01	
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2778&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2779&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_277A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_277B&MI_06
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2782&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_0C03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2010&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_201B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2028&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2D01&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2D03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2D05&MI_02

%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9031&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9091&MI_03
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D

;mtk
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2003&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2005&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2006&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2010&MI_02
%SingleAdbInterface%        = USB_Install, USB\VID_0E8D&PID_201C
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_201D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_201B&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_0E8D&PID_2024
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2025&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2026&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2027&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2028&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_202E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_202F&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2030&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2040&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2041&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2044&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2061&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2062&MI_02

;C2K related
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2032&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2034&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2035&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2037&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2039&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2050&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2053&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2054&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2063&MI_07
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2064&MI_02


;MIDI related
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2048&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2049&MI_02

;MBIM related
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2056&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2057&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_2059&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0E8D&PID_205F&MI_01
;mtk end 

;oppo copy from mtk
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2003&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2005&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2006&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_200E&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2010&MI_02
%SingleAdbInterface%        = USB_Install, USB\VID_22D9&PID_201C
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_201D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2014&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2017&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2019&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_201B&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_22D9&PID_2024
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2025&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2026&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2027&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2028&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2029&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_202E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_202F&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2030&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2040&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2041&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2044&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2061&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2062&MI_02

;C2K related
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2032&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2034&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2035&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2037&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2039&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2050&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2053&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2054&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2063&MI_07
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2064&MI_02


;MIDI related
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2048&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2049&MI_02

;MBIM related
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2056&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2057&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2059&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_205F&MI_01
;;oppo copy from mtk end 

;oppo new add
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90B4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90B6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_903A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9060&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9082&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_908C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90D1&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_901F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90B8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_90D3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2767&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2006&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_2D03&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2048&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2049&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2032&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2034&MI_03
%SingleBootLoaderInterface% = USB_Install,USB\VID_18D1&PID_4EE2&MI_01
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE2&REV_0409&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE9&MI_02
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0&REV_0414
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0
	
;oppo new add end 

;Unisoc add SPRD Adb
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4002&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4003&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4012&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4013&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4022&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4023&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4026&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4028&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4029&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4030&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4032&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4033&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_4D01&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5A5B&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D01&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D04&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D06&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D21&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D23&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D24&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D25&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D27&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D29&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D31&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_5D34&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A002&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A002&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A012&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A012&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_A022&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_A022&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD21&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD21&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_AD24&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_1782&PID_AD24&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D001
%CompositeAdbInterface%      = USB_Install, USB\VID_1782&PID_D002
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4002&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4003&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4012&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4013&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4022&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4023&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4026&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4028&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4029&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4030&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4032&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4033&MI_04
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4D01&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5A5B&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D01&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D04&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D06&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D21&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D23&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D24&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D25&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D27&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D29&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D31&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_5D34&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_A002&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_A002&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_A012&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_A012&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_A022&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_A022&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_AD21&MI_02
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_AD21&MI_03
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_AD24&MI_01
%CompositeAdbInterface2%     = USB_Install, USB\VID_22d9&PID_AD24&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_D001
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_D002
; GOOGLE Adb
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_0FFF
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D06&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D07&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_2D08&MI_01
%SingleBootLoaderInterface%  = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE7&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_18D1&PID_4EE8&MI_00
%SingleBootLoaderInterface%  = USB_Install, USB\VID_22d9&PID_0FFF
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_2D06&MI_02
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_2D07&MI_01
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_2D08&MI_01
%SingleBootLoaderInterface%  = USB_Install, USB\VID_22d9&PID_4EE0
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_200E&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_200E&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4EE7&MI_00
%CompositeAdbInterface%      = USB_Install, USB\VID_22d9&PID_4EE8&MI_00

;add plus
;14041
%SingleAdbInterface%        = USB_Install, USB\VID_22D9&PID_2769
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2769&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_276D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9031&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2765&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2766&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2767&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2772&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2774&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_22D9&PID_2775&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9025&MI_01
;14049
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D       ;fastboot
%SingleBootLoaderInterface% = USB_Install, USB\VID_2A70&PID_D00D       ;oem fastboot
%SingleAdbInterface%        = USB_Install, USB\VID_2A70&PID_4EE7       ;adb
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9031&MI_02 ;default
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9091&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9039&MI_01 ;mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_904E&MI_01 ;ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9011&MI_02 ;mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9012&MI_02 ;mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_901C&MI_00 ;adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_05C6&PID_9015&MI_01 ;mtp,adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_2A70&PID_9024&MI_02 ;rndis,adb

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName                = "OPLUS, Inc."
SingleAdbInterface          = "Android ADB Interface"
CompositeAdbInterface       = "Android Composite ADB Interface"
CompositeAdbInterface2      = "Android Composite ADB Interface2"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Phone"
